Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*c-2 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 6A | Mitsubishi FX connection cable by Pro-face CA3-CBLFX/1M-01 (1m) or CA3-CBLFX/5M-01 (5m) + Function extension board by Mitsubishi Electric Corp.*5 FX1N-422-BD, FX2N-422-BD, FX3U-422-BD or FX3G-422-BD |
GP-4116 (COM1) | 6B | Mitsubishi PLC FX Series CPU I/F Cable by Pro-face ZC9CBFX11 (1m) or ZC9CBFX51 (5m) + Function extension board by Mitsubishi Electric Corp.*5 FX1N-422-BD, FX2N-422-BD, FX3U-422-BD or FX3G-422-BD |
PS5000 PS6000 (Optional Interface) PSA6000 *6 | 6C | Mitsubishi PLC FX Series CPU I/F Cable by Pro-face ZC9CBFX11 (1m) or ZC9CBFX51 (5m) + Function extension board by Mitsubishi Electric Corp.*5 FX1N-422-BD, FX2N-422-BD, FX3U-422-BD or FX3G-422-BD |

*c-2Except ST-6200

*5Supported function extension boards vary depending on the model.

CPU | Function Extension Board
FX1S, FX1N | FX1N-422-BD
FX2N | FX2N-422-BD
FX3U, FX3UC | FX3U-422-BD
FX3G, FX3S | FX3G-422-BD

*6Only the COM port which can communicate by RS-422/485 (4 wire) can be used.

IPC COM Port