### MICRO-EHV Series

Device | Bit Address | Word Address | Double Word Address | 32 bits | Remarks
--- | --- | --- | --- | --- | ---
External Input | X0000-X0039 | WX000-WX002 | DX000 |  | *1
External Output | Y0100-Y0123 | WY010-WY011 | DY000 |
Inner Output | R000-R7BF | - | - |
Special Inner Output | R7C0-RFFF | - | - |
Data Area | M0000-M7FFF | WM000-WM7FF | DM000-DM7FE |
On Delay Timer | TD0000 - TD2047 | - | - |
Off Delay Timer | TDN0000-TDN2047 |  |  |
Single-shot Timer | SS0000-SS2047 | - | - |
Watchdog Timer | WDT0000-WDT2047 | - | - |
Mono Stable Timer | MS0000-MS2047 | - | - |
Retentive Timer | TMR0000-TMR2047 | - | - |
Up-down Counter | CT000-CT511 | - | - |
Up Counter | CU000-CU511 | - | - |
Ring Counter | RCU000-RCU511 | - | - |
Timer Counter (Elapsed Value) | - | TC0000-TC2047 | - |
Word Inner Output | WR0000.0-WR7FFF.F | WR0000-WR7FFF | DR0000-DR7FFE |
Word Special Inner Output | WRF000.0-WRF1FF.F | WRF000-WRF1FF | DRF000-DRF1FE |

*1Write disable

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms