### External Device Settings

Use the ladder software (KV STUDIO Ver. 4 or later) for External Device communication settings. Refer to your External Device manual for details.

1. Start up the ladder software.

2. From the [File] menu, select [New Project] and display the [New Project] dialog box.

3. Type a project name in [Project Name], select the External Device to use under [PLC model], and click [OK].

4. Click [Yes] in the [Confirm unit setting information] dialog box and display the [Unit Editor] window.

5. Select "KV-LE20V" from the displayed unit list on the [Select unit] tab, and drag & drop it to the unit placement area.

6. Right-click "KV-LE20V" in the unit placement area and select [Unit setup display].

7. Configure the following setting items.

   Setup Items | Settings
   First DM No. | DM10100
   Speed | 100/10 Mbps (automatic)
   IP Address | 192.168.0.1
   Subnet Mask | 255.255.255.0
   Port No. (HOST Link) | 8501

8. From the [Convert] menu, select [Auto-assign relay/DM].

9. From the [File] menu, select [Close] and display the [Unit Editor] dialog box.

10. Click [Yes].

11. From the [Monitor/Simulator] menu, select [Transfer to PLC] to display the [Transfer Program] dialog box.

12. Check [Unit setting info] and [Program], and then click [Execute]. The setting information is transferred.

This completes the setting of the External Device.

NOTE

- Check with your network administrator about the IP address you want to use.
- Do not duplicate IP addresses on the same network.