Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 3G | User-created cable | Cable length: 500m or less
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 3I | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + User-created cable | Cable length: 500m or less
3A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + User-created cable
3B | User-created cable
PS5000 PS6000 (Optional Interface) PSA6000 *4 | 3K | User-created cable | Cable length: 500m or less

*b-3Except ST-6200 *4Only the COM port which can communicate by RS-422/485 (2 wire) can be used. IPC COM Port

IMPORTANT:

- Terminal number used for communication differs depending on the External Device series.
  Terminal numbers corresponding to each series are shown below. SG terminals are not available for these series. Apply masking using insulation tape, etc. Implement Type D installment to the shield connected to the FG.

  Series | + | -
  --- | --- | ---
  PXG4 | 7 | 8
  PXG5/PXG9 | 1 | 2
  PXR3 | 15 | 14
  PXR4/PXR7 | 7 | 8
  PXR5/PXR9 | 1 | 2

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.