### H5U Series

Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | X0000 - X1777 | - |  |
Output Relay | Y0000 - Y1777 | - |
Internal Relay | M0000 - M7999 | - |
State Relay | S0000 - S4095 | - |
Internal Relay | B00000 - B32767 | - |
Data Register | - | D0000 - D7999 |
Extension Register | - | R00000 - R32767 |

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms

####