### External Device Settings

Use Smart Loader Package (SLP-NX) for the External Device communication settings.

Refer to your External Device manual for details.

1. Start Smart Loader Package.

2. Display the configuration screen of the External Device.

3. Execute scanning of the External Device.

   The External Device being connected via network are displayed on the configuration screen.

NOTE

- The factory default IP address of the External Device is 192.168.255.254. If no External Device is displayed on the screen, use Smart Loader Package and adjust the PC's IP address.

4. Set the External Device IP address as follows:

   Setup Items | Setting
   IP Address | 192.168.0.1

5. Transfer the settings to the External Device.

NOTE

- Check with your network administrator about the IP address you want to use.
- Do not duplicate IP addresses on the same network.