### External Device Settings

Use the ladder software (LOGO!Soft Comfort V8.0/V8.1) to configure the External Device communication settings. Please refer to the External Device manual for details.

NOTE

- The version of ladder software depend on the External Device to be used. Please refer to the manual of the External Device for more details.

1. Start up the ladder software.

2. Create the ladder diagram.

3. From the [Tools] menu select [Ethernet connections], and define the setup items as follows:

   Setup Items | Setup Description
   --- | ---
   IP address | 192.168.0.1
   Subnet mask | 255.255.255.0
   Gateway | 192.168.0.10

4. From [Ethernet connections], right-click [Ethernet Connections] and from the shortcut menu select [Add server connection].

5. In [Local Properties (Server)], select the [Connect with an Operator Panel (OP)] and [Accept all connection requests] check boxes. In [Remote Properties (Client)], set [TSAP] to "02.00".

6. Click [OK] to close the dialog box.

7. Update the Parameter VM Mapping and then download the communication setting to the External Device.

NOTE

- Connection is lost when there is no communication between the Display and the External Device after 9 seconds. A time-out error is displayed as the connection is lost, when the Display tries to reconnect. The time-out error is restored automatically.
  To prevent the time-out error from being displayed, make the settings so that communication may be performed in a shorter cycle than the specified time-out for connection, using a watchdog timer, and etc.