### Supported Device

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Input / Output Relay | P000 - P63F | P00 - P63 |  |
Auxiliary Relay | M0000 - M191F | M000 - M191 |
Keep Relay | K000 - K31F | K00 - K31 |
Link Relay | L000 - L63F | L00 - L63 |
Special Relay | F000 - F63F | F00 - F63 | *1
Timer (Contact) | T000 - T255 | ----- |
Counter (Contact) | C000 - C255 | ----- |
Timer (Elapsed Value) | ----- | T000 - T255 |
Counter (Elapsed Value) | ----- | C000 - C255 |
Step Controller | ----- | S00 - S99 |
Data Register | ----- | D0000 - D9999 |

*1Write disable.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms