### Settings of External Device

Use the LS ELECTRIC setting tool (XG-PD Editor) to configure communication settings for the External Device.

Refer to your External Device manual for details.

1. Start up the setting tool.

2. From the [File] menu, select [New File] and create the XGB project.

   NOTE

   - To read the project from the External Device, select [Open from PLC...].

3. From the [Online] menu, select [Connect].

4. From the [Online] menu, select [Read IO Information].

5. In the [Standard settings] tab, double-click [Cnet] to display the [Standard Settings-Cnet] dialog box.

6. Set the [Channel 2] setup items as follows, and click [OK].

   Setup Item | Setting Value
   --- | ---
   Type | RS232C
   Speed | 38400
   Data Bit | 8
   Stop Bit | 1
   Parity Bit | NONE
   Modem Type | Null Modem
   Station | 0
   Active mode | XGT server

7. From the [Online] menu, select [Write Parameter] to display the [Write Parameter] dialog box.

8. Select the module to use, and click [OK].

9. From the [Online] menu, select [Reset].