### 3G

1:1

1:n

Legend | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal Block External Device side: Terminal Block |

IMPORTANT:

- Use the lead wire to connect between "-" terminal and "E" terminal in the External Device which terminates the connection.

NOTE

- Cable length: 1200m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON