### 3H

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal Block External Device side: Half pitch 14 pin | Connect the shield to FG (Shell).

NOTE

- We recommend following connector and case on the External Device side.
  Connector: HDR-E14MAG1+ by HONDA TSUSHIN KOGYO CO., LTD.
  Case: HDR-E14LPA5 by HONDA TSUSHIN KOGYO CO., LTD.
- Cable length: 30m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON