### Setting of External Device

Use the rotary switch on the front of the unit to set the mode switch. Use the ladder software to set other switches than the mode switch. Please refer to Sample of Ladder Program for the sample ladder to write the initial data.

Setup Items | Setup Description
--- | ---
Mode Switch | 0
Active Open | 0: Not request
PING Request | 1: Request
Source Node IP Address | 192.168.0.1
Source Node Port No. | 401 (HEX)
Use Other Node Table | Use
Connection | Protocol Open Method | 0100H
Other Node Table No. | Preset other node table No.
Other Node Table | CPU Operation Mode | PC3
Other Node IP Address | Set IP address of the Display.
Other Node Port No. | Set the port No. of the Display.

##### Example of Ladder Program

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.
- Please refer to the manual of the External Device for more details.