### External Device Settings

Depend on the specification of External Device.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address

NOTE

- The device storage order of data varies depending on the External Device. Change the String Mode to match the device order same as a External Device.

NOTE

- When using 1785-ENET, it must be series A rev.D, or series B rev.A, or later.
- When connecting to the CPU directly, flash upgrade the firmware to CIP series E rev.D.1, series D rev.E.1, series C rev.N.1, or later.