### External Device Settings (Ethernet communication port on EH-R2LH)

Use the EH remote slave station IP address setting tool (Version 1.00) for communication setting.

Please refer to the manual of the External Device for more details.

1. Set [INIT] of the mode setting SW on the slave station communications module to the "ON" position.

NOTE

- When [INIT] of the mode setting SW is set to "ON", settings are temporarily changed to following contents.

  Setup Items | Setting
  --- | ---
  IP Address | 192.168.0.1 (Fixed)
  Subnet Mask | 255.255.255.0
  Default Gateway | 0.0.0.0
  Logic Port | 3004
  Communications Protocol | UDP/IP
  Timeout Setting | None

2. Turn on the power.

3. Start up the EH remote slave station IP address setting tool.

4. Click [Connect] and read out the current setting values.

IMPORTANT:

- To access, PC’s IP address up to the third octet must be set to 192.168.0. (192.168.0.10, etc.)

5. Set each item as follows:

- IP Address Setting

  Setup Items | Setting
  --- | ---
  IP Address | 192.168.0.1
  Subnet Mask | 255.255.255.0
  Transmission Speed/System | AUTO

- Logic Port No. Setting (Port1)

  Setup Items | Setting
  --- | ---
  Port No. | 3004
  Protocol | UDP/IP

6. Click [Set].

7. Confirm the setting complete message and press [OK].

8. Turn OFF the power of the External Device. After setting OFF [INIT] of the mode setting SW on the slave station communications module, turn ON the power of the External Device.

NOTE

- Check with a network administrator about IP address. Set up unique IP addresses on the same network.

NOTE

- The following CPU ROM versions are required to use the remote communications module.

CPU | Supported versions
EHV-CPU128 | ROM Ver.0117 or later
EHV-CPU64 | ROM Ver.1117 or later
EHV-CPU32 | ROM Ver.2117 or later
EHV-CPU16 | ROM Ver.3117 or later

NOTE

- EH-RMAH is required to use EH-R2LH.