### Setting of External Device

Use the the ladder software (PCWin) to set up the External Device communication settings.

Please refer to the manual of the External Device for more details.

1. Start the ladder software and create a project.

2. In the project tree, set the [CPU Mode] to [PC10 mode].

3. In the project tree, double-click [Link Parameter].

4. In the [Link parameter setup] dialog box, select the link number of the link module you want to define, and click [Link setup].

5. Define the following settings and click [OK].

   Setup Items | Settings
   --- | ---
   Rack No. | Built-in
   Slot No. | Standard
   Link module name | Computer link

6. Select the link module, click [Detail] and define the following settings.

   Setup Items | Settings
   --- | ---
   Station No. | 00
   Data bits | 8bits
   Stop bits | 1bit
   Bits per second | 19200bps
   2-wire/4-wire | 2-wire

7. Write the communication settings to the External Device. After the write operation is complete, restart the External Device.