Display (Connection Port) | Cable | Remarks
--- | --- | ---
GP-4116 (COM1) | 2E | User-created cable | Cable length: 1000m or less.
SP-5B10 (COM1/2) SP-5B90 (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) | 2G | RS-422 terminal block conversion adapter by Pro-face PFXZCBADTM1 + User-created cable | Cable length: 1000m or less.
2A | COM port conversion adapter by Proface CA3-ADPCOM-01 + Connector terminal block conversion adapter by Proface CA3-ADPTRM-01 + User-created cable
2B | User-created cable

*b-3Except ST-6200

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.