### Setting of External Device

Use the configuration tool (S10V BASE SYSTEM) for communication settings of the External Device.

1. Set the [ST No.] rotary switch on the CPU unit to "0,0", and then activate the External Device.

2. Connect an RS-232C cable from your PC to the CPU unit of the External Device, and then start up the configuration tool.

3. Click [ONLINE] of [Connection status].

4. Click [Set IP Address] of [CMU].

5. Set the communication settings in the [Set IP Address] dialog box displayed.

   Setup Items | Setup Description
   --- | ---
   Module | ET.NET (Main)
   IP Address | 192.168.0.1
   Subnetmask | 255.255.255.0

6. Restart the External Device.

NOTE

- For LQP520, LQP510 is also required.