Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 30G | User-created cable | Cable length: 15m or less.
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 30I | RS-422 terminal block conversion adapter by Pro-face PFXZCBADTM1 + User-created cable | Cable length: 15m or less.
30A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Connector terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + User-created cable
30B | User-created cable
PS5000 PS6000 (Optional Interface) PSA6000 *5 | 30K | User-created cable | Cable length: 15m or less.

*b-3Except ST-6200 *5Only the COM port which can communicate by RS-422/485 (2 wire) can be used. IPC COM Port

NOTE

- The shield of cables connected to FX2N-485-BD, FX1N-485-BD, FX2NC-485ADP and FX3U-485ADP must be D-class grounded.
- Connect the shield of cable connected to FX0N-485ADP to the adapter FG terminal. In addition, always connect the FG terminal of FX0N-485ADP to the ground terminal of External Device body with D-class grounded.
- FX3U-485-BD, FX3U-485ADP and FX3G-485-BD have built-in termination resistance. Use the termination resistance switch to set termination resistance.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.