### Inverter

Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Bit Register*1 | BR0000.0 - BR195C.F | ------ | - | *2
Register*1 | ------ | 0000 - 195C |  |

*1The Bit Register and the Register are the same device, but their bit write operation differs. Use either as needed. *2When bits are written, the Display reads the corresponding word address from the External Device, sets particular bits of that word address to ON, and then returns the resulting address to the External Device. Note that the data may not be written correctly if you write to the word address using the ladder program while the Display is reading data from, and writing data to, the External Device. To write bits to the write-only register, use a registering device. Writing bits to the write-only register will cause a communication error to appear when the readout command is executed.

NOTE

- If you use a device, set the address to the MEMOBUS register No. corresponding to the parameter No. Refer to your External Device manual for details.
  Example) Correspondence between the Inverter Constant Number and MEMOBUS register

- Constant No. | Name | MEMOBUS Register
  A1-02 | Selection of Control Mode | 102H
  b1-01 | Selection of frequency command | 180H

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms