### 3G)

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: Depends on the specification of the External Device. |

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON

For the Displays other than that used as the terminal, set the DIP Switch 1-4 on the rear of the Display to OFF in the 1:n connection.