### MELSEC L Series

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Input Relay | X0000-X1FFF | X0000-X1FF0 |  |
Output Relay | Y0000-Y1FFF | Y0000-Y1FF0 |
Internal Relay | M00000-M61439 | M00000-M61424 |
Special Relay | SM0000-SM2047 | SM0000-SM2032 |
Latch Relay | L00000-L32767 | L00000-L32752 |
Annunciator | F00000-F32767 | F00000-F32752 |
Edge Relay | V00000-V32767 | V00000-V32752 |
Step Relay | S0000-S8191 | S0000-S8176 |
Link Relay | B0000-BEFFF | B0000-BEFF0 |
Special Link Relay | SB0000 - SB7FFF | SB0000 - SB7FF0 |
Timer (Contact) | TS00000-TS25471 | - |
Timer (Coil) | TC00000-TC25471 | - |
Retentive Timer (Contact) | SS00000-SS25471 | - |
Retentive Timer (Coil) | SC00000-SC25471 | - |
Counter (Contact) | CS00000-CS25471 | - |
Counter (Coil) | CC00000-CC25471 | - |
Timer (Current Value) | - | TN00000-TN25471 |
Retentive Timer (Current Value) | - | SN00000-SN25471 |
Counter (Current Value) | - | CN00000-CN25471 |
Data Register | - | D000000-D421887 |
Special Register | - | SD0000-SD2047 |
Link Register | - | W00000-W66FFF |
Special Link Register | - | SW0000-SW6FFF |
Module Access Device | - | U000-G00000-U1FF-G65535 | *2
File Register (Normal) | - | R00000-R32767 | *1
File Register (Block switching is not necessary) | - | ZR000000-ZR393215 | *1
File Register (0R - 11R) | - | 0R0000-0R32767 | *1
- | 1R0000-1R32767
- | 2R0000-2R32767
: | :
- | 10R0000-10R32767
- | 11R0000-11R32767

*1It is different by the memory card which uses the range of file register.

*2Device for accessing SLMP compatible devices, as well as the intelligent function unit’s buffer memory. The first three digits of the address specifies the intelligent module’s starting I/O number.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms