### Settings of External Device

Use the mode switch on the link I/F and the setting tool (Cnet Frame Editor) to configure communication settings for the External Device.

Refer to your External Device manual for details.

##### Mode Switch

- When using G6L-CUEB/G6L-CUEC.

  Rotary Switch | Setting Description
  --- | ---
  1 | Dedicated

- When using G3L-CUEA/G4L-CUEA.

  Rotary Switch | Setting Description
  --- | ---
  1*1 | Dedicated

*1 Set to 1, when using in the External Device Interlocking mode.

Set to 3, when using in the External Device Stand-alone mode.

##### Setting Tool

1. Start up the setting tool.

2. Set [channel] and [Basic Parameters] setup items as follows.

Setup Item | Setting Value
--- | ---
Channel | RS422 side
Station | 0
Type | Null Modem
Baud Rate | 38400
Data Bit | 8
Parity | None
Stop Bit | 1
Monitor Entry | 16x20

3. Transfer the setting contents to External Device.