### Setting of External Device

Use the ladder software "PL7-07" for communication settings on External Device.

Go to [Configuration] in [Application Browser], [Hardware Configuration] and [Comm] in this order in "PL7-07", and perform the communication settings as below.

Setup Items | Setup Description
--- | ---
CHANNEL | CHANNEL 1
TSX SCP 114 RS485 MP PCMCIA CARD
UNI-TELWAY LINK
Type | Master
Trasmission Speed | 19200
Data | 8 bits
Parity | Odd
Stop | 1 bit
Number of Slaves | 8

NOTE

- Do not set the address which exceeds "Number of Slaves" on External Device in Server Address and Clients Address. If you set the address which exceeds "Number of Slaves" in Server Address and Clients Address, timeout error will occur, which disables the communication with the External Device. In addition, when you connect many client devices (Display/External Device) on the same serial network, set the longer timeout on the Display.