### 5E

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal Block External Device side: D-Sub 25 pin (plug) |

NOTE

- As the External Device has the termination resistance built-in, you do not need to connect the termination resistance.
- Cable length: 500m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | OFF