### 5A

1:1

1:n

Legend | Name | Note
--- | --- | ---
(1) | COM port conversion adapter by Pro-face CA3-ADPCOM-01 |
(2) | Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 |
(3) | User-created cable Connector Display side: Terminal Block External Device side: Terminal Block |

NOTE

- Use the DIP switch in the communication cassette to set the termination resistance. Set SW1-1 of the External Device which terminates the connection to ON.
- Cable length: 1200m or less.