### 1H)

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: D-sub 9 pin (plug) External Device side: Terminal Block |
(2) | RS485 master cable by Sanmei Electronics Co., LTD. Si-RSM**M | Connect the cable to RM connector on External Device.
(3) | RS485 slave cable by Sanmei Electronics Co., LTD. Si-RSS | Connect one side of the cable to RS connector on External Device that's situated nearer Display. Connect the other side of the cable to RM connector on next External Device.

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power for the Siemens AG's PROFIBUS connector. Do not use it for other devices.

NOTE

- Cable length: 20m or less.