### 3A)

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9pin (Socket) External Device side: Half-pitch 20pin (Plug) | Instead of connecting the Display (FG), connect the Shield to the Shell.

NOTE

- Cable length: 15m or less.

*1 When connecting with 30i-Model A, 31i-Model A or 32i-Model A, The pin number of SG changes with ports to be used.

Use port | Pin No. of SG
--- | ---
JD36A | 8
JD54 | 4