### 5H

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | Distributor BMJ-8P |
(2) | Distributor BMJ-8 |
(3) | User-created cable • Connector Display side: D-sub 9 pin (plug) Distributor side: RJ45 connector External Device side: RJ45 connector | Connect the shield to FG (Shell).

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power for the Siemens AG's PROFIBUS connector. Do not use it for other devices.

NOTE

- Total cable length: 500m or less