Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) STM6000 (COM1) PC/AT IPC*2 | 6A | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB | Cable length from Display to SIO converter: 15m or less Cable length from SIO converter to External Device: 100m or less
6B | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
6C | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Junction by AMP 5-1473574-4 + User-created cable 3 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
6D | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Junction by AMP 5-1473574-4 + User-created cable 3 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB | Cable length from Display to SIO converter: 15m or less Cable length from SIO converter to External Device: 100m or less
6E | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Insulated PIO terminal block by IAI Corporation RC*-TU-PIO-* + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO***-H6 or CB-ERC-PWBIO***-RB-H6
GP-4115 (COM1) | 6F | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB | Cable length from Display to SIO converter: 15m or less Cable length from SIO converter to External Device: 100m or less
6G | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
6H | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Junction by AMP 5-1473574-4 + User-created cable 3 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
6I | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Junction by AMP 5-1473574-4 + User-created cable 3 + Terminal block + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO*** or CB-ERC-PWBIO***-RB
6J | User-created cable 1 + SIO converter by IAI Corporation RC*-TU-SIO-* + User-created cable 2 + Insulated PIO terminal block by IAI Corporation RC*-TU-PIO-* + Power & I/O Cable by IAI Corporation CB-ERC-PWBIO***-H6 or CB-ERC-PWBIO***-RB-H6

*2Only the COM port which can communicate by RS-232C can be used.

IPC COM Port

NOTE

- When connecting to 3 or more External Devices, use link connection terminal block or junction by AMP.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.