### External Device Settings

Use Studio 5000 (former RSLogix5000) for communication setting.

Please refer to the manual of Studio 5000 for more details.

1. Select [New Module] from the menu displayed by right-clicking [I/O Configuration] in the Project tree of Studio 5000.

2. Select a module in the [Select Module] dialog box and click [OK].

3. Select [Properties] from the menu displayed by right-clicking the module added in the Project tree.

4. Use the [General] tab to set IP address and other items.

5. Download the setting in the External Device and restart the External Device.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.

NOTE

- The device storage order of data varies depending on the External Device. Change the String Mode to match the device order same as a External Device.

NOTE

- Select Control/Compact/Flex Logix Native when using Native tag names on External Devices.
- Refer to the following for the CPU that generates a controller tag of Embedded I/O when the L5K file is imported.
  "Data Type Defined Module List"