Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Input Relay | X00201 to X71664 | X00201 to X71649 |  | *1*2
Output Relay | Y00201 to Y71664 | Y00201 to Y71649 | *1
Internal Relay | I00001 to I65535 | I0001 to I65521 |
Common Relay | E0001 to E4096 | E0001 to E4081 |
Special Relay | M0001 to M9984 | M0001 to M9969 |
Link Relay | L00001 to L78192 | L00001 to L78177 | *3
Time-up Relay | TU0001 to TU3072 | --- |
Count-up Relay | CU000 to CU3072 | --- |
Timer present value | --- | TP0001 to TP3072 |
Timer present value (count-up) | --- | TI0001 to TI3072 |
Timer preset value | --- | TS0001 to TS3072 | *2
Counter present value | --- | CP0001 to CP3072 |
Counter present value (count-up) | --- | CI0001 to CI3072 |
Counter preset value | --- | CS001 to CS3072 | *2
Data Register | D00001.00 to D65535.15 | D00001 to D65535 |
Common Register | B000001.00 to B262144.15 | B000001 to B262144 |
Cache Register | F000001.00 to F524288.15 | F000001 to F524288 | *4
General Register | R0001.00 to R4096.15 | R0001 to R4096 |
Special Register | Z0001.00 to Z1024.15 | Z0001 to Z1024 |
Link Register | W00001.00 to W78192.15 | W00001 to W78192 | *3
Special Module | --- | SW0010000 to SW7169999 | *2*5
Information | --- | INF100 to INF101 |  | *2*6
--- | INF200 to INF214 | *2*6
--- | INF30010 to INF37163 | *2*6
INF4100.00 to INF4215.15 | INF4100 to INF4215 | *2*6
--- | INF500 | *6
Program Information | --- | PRI00000 to PRI99913 | *2*7
User Log Read | --- | ULR000000 to ULR 064128 | *2*8
Error History Read | --- | ERH000000 to ERH 128000 | *2*9

*1Address for input relay and output relay can be specified when data position number (bit) 01 to 49 for lower 2 digits is the value of (multiples of 16) + 1 only.

Example: X00201

*2 Write disable

*3In link relay (L) and link register (W), the upper 1st digit on address input area shows the link number, and lower 4th digit shows the address. Specify the word address for link relay (L) and link register (W) with the value of (multiples of 16) + 1.

Example: When specifying L71024 of link relay

*4Only the F3SP71-4N, F3SP76-7N, F3SP71-4S and F3SP76-7S can be used.

*5Information of Special Module Read/Write

*6Information Read
1. Read the status of CPU module and program

2. Read the information of system ID, CPU type and area size

3. Read the mounting module name

4. Read the ERR LED of CPU module or the ALM LED lighting factor

5. Delete the current alarm information of CPU module (write only)

*7Program Information Read

*8User Log Read

*9Error History Read

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms