### Setting Example

Use the Control Techniques configuration tool (CTSoft Ver.01.10.02) for External Device communication settings. Refer to your External Device manual for details.

1. Start up the configuration tool.

2. Create a project and display [My Drive 1] and [My Drive 2] in the tree view.

   NOTE

   - When using CTNet, two or more Drives are required. In this section, the Drive is referred to as [My Drive 1] and [My Drive 2].

3. From [Parameters] select [SM-Applications Plus] for the slot number to use under [My Drive 1] and [My Drive 2] in the tree view, and display the dialog box.

4. Double-click a parameter you want to set and display the [Edit Parameter] dialog box.

5. Set each item as shown below and click [OK]

   Parameter | Setup Items | Setting
   --- | --- | ---
   My Drive 1 | My Drive 2
   22 | CTNet token ring ID | 0 | 0
   23 | CTNet node address | 1 | 255
   24 | CTNet baud rate | 2.5 | 2.5

   NOTE

   - Use parameters 25 to 35 as default.

6. Download the communication settings to the External Device.

7. Reset the External Device.

8. Save the communication settings in the External Device.

NOTE

- Use an integer from 1 to 247 to enter the unit ID of the External Device.