### Setting of External Device

Use the GPP function software by Mitsubishi Electric Corporation to perform the communication settings as below.

1. Double-click [PC Parameter] from [Parameter] to select the [I/O Assign Setting] tab.

2. Click [Type] to select [Intelligent].

3. Click [Switch Settings] and set as below.

   Setting Switch | Setting Value | Setup Description
   Switch 3 | 07E6 | Transmission Speed = 19200 Data Length = 8 With/Without Parity = With Parity = Odd parity Stop Bit = 1 Sum Check = Enable
   Switch 4 | 0005*1 | Mode = Form 5
   Switch 5 | 0000 | Station No. = 0

*1Set the value according to [Format] to be used.

NOTE

- Please refer to the manual of the External Device for more detail on setting description.

##### Important Item

When you use 2 types of interface in QJ71C24, please set the total speed of CH1 and CH2 to 115200 or less.

NOTE

- The unit (QJ71C24N, QJ71C24N-R2 and QJ71C24N-R4) whose first 5 digits of the serial No. is less than "10042" cannot be connected with the universal model built-in Ethernet port QCPU.