### Settings of External Device

Use the TwinCAT for communication settings of the External Device. Please refer to the manual of the External Device for more details.

1. Set up the External Device as in the following table. Please refer to the manual of the External Device for more details.

   Setup Items | Setting Value
   --- | ---
   Address | 192.168.0.1
   AMS Net Id | 192.168.0.1.1.1

2. Change the target to External Device.
   From the TwinCAT System Manager's tree view, select [SYSTEM - Configuration].

3. From the [General] tab, click [Choose Target] to display a dialog box. Select the External Device. When selecting the target, set the [Target Route] and [Remote Route] to [Static].

4. Set up the Display's IP address and AMS NetId on the External Device.
   From the TwinCAT System Manager's tree view, select [SYSTEM - Configuration] and then [Route Settings] to display a screen.

5. Select the [Static Route] tab and click [Add].

6. Enter the following settings and click [Add Route].

   Setup Items | Setting Value
   --- | ---
   AmsNetId | 192.168.0.2.1.1
   Transport Type | TCP/IP
   Address Info | 192.168.0.2 (IP Address)
   Target Route | Static
   Remote Route | none

7. Create the project in TwinCAT PLC Control, and download to the External Device.

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address in the same network.