### R7G4HML3-LC2A(M-III) Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Auto-Zero | - | AZ0/00 - AZ1/00 |  | *1 *2
Zero point adjust | - | ZPA0/00 - ZPA1/00 | *1 *2
Span point adjustment | - | SPA0/00 - SPA1/00 | *1 *2
Average cycle | AC0/00.0 - AC1/00.F | AC0/00 - AC1/00 | *2 *3
Monitor Output | - | MO0/00 - MO1/00 | *1 *2
Monitor Output Release | - | MOR0/00 - MOR1/00 | *1 *2
Offset Reset | - | OR0/00 - OR1/00 | *1 *2
Virtual Memory Space | - | M0/0000-M0/019C | *4 *5
CR Filter Set | CR0/00.0 | CR0/00 | *3

*1Read disable.

*2When a value is written, the corresponding processing is run.
The address consists of the address part and the channel part.

*3When you write to the bit address, the Display reads the entire word, sets the defined bit, then returns the new word value to the External Device. If the ladder program writes data to this word address during the bit write process, the resulting data may be incorrect

*4Write disable

*532-bit device

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms