### 5G

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: Uni-Telway cable |
(2) | Uni-Telway cable by Schneider Electric Industries TSX SCP CU 4030 (3m) |
(3) | PCMCIA card for RS485 by Schneider Electric Industries TSX SCP 114 |

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON