Connection Configuration

Communication Settings

Supported Devices

## Connection Configuration

NOTE

- This driver allows an External Device conforming to CoDeSys Automation Alliance to be connected. We have confirmed the connections of the External Device which listed in Maker List.

- 1:1 Connection

- 1:n Connection

NOTE

- Maximum number of External Devices is 64.

- 1:n Connection (Gateway connection)

NOTE

- Maximum number of External Devices is 64.

- n:1 Connection

NOTE

- The number of Displays you can connect depends on the External Device. Check the specifications of the External Device.

- n:m Connection

NOTE

- Maximum number of External Devices is 64.

- The number of Displays you can connect depends on the External Device. Check the specifications of the External Device.

## Communication Settings

Examples of communication settings of the Display and the External Device, recommended by Pro-face, are shown.

WARNING

UNINTENDED EQUIPMENT OPERATION

Read and understand the instructions in this section to ensure data is properly transferred.

## Supported Devices

Range of supported device address is shown in the table below. Please note that the actually supported range of the devices varies depending on the External Device to be used. Please check the actual range in the manual of your External Device.

You can import tag data from the project created by your programming software.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Do not simultaneously write to the same register from Display and External Device program.
- Do not write 16-bit word values to registers being accessed in a bitwise manner.