### Q Series Motion Controller (Q***HCPU)

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Input Relay | X0000-X1FFF | X0000-X1FF0 |  |
Output Relay | Y0000-Y1FFF | Y0000-Y1FF0 |
Internal Relay | M00000-M08191 | M00000-M08176 |
Special Relay | SM0000-SM0255 | SM0000-SM0240 |
Latch Relay | L00000-L08191 | L00000-L08176 |
Annunciator | F00000-F02047 | F00000-F02032 |
Link Relay | B0000-B1FFF | B0000-B1FF0 |
Data Register | ------ | D0000000-D0008191 |
Special Register | ------ | SD0000-SD0255 |
Link Register | ------ | W0000-W1FFF |
Motion Register (#)*1 | ------ | %MR0000-%MR8191*2 |

*1No. 2 to No. 4 can be allocated to the motion CPU.

*2Device name with motion CPU is #.

NOTE

- The notation of addresses differs depending on a selected Unit No.
  <Ex.>When 0 is selected for Unit No.,

  <Ex.>When 1 is selected for Unit No.,

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms