### MELSEC Q (High performance model) Series

Device | Bit Address | Word Address | 32bits | Remarks
--- | --- | --- | --- | ---
Input Relay | X0000-X1FFF | X0000-X1FF0 |  |
Output Relay | Y0000-Y1FFF | Y0000-Y1FF0 |
Internal Relay | M00000-M32767 | M00000-M32752 |
Special Relay | SM0000-SM2047 | SM0000-SM2032 |
Latch Relay | L00000-L32767 | L00000-L32752 |
Annunciator | F00000-F32767 | F00000-F32752 |
Edge Relay | V00000-V32767 | V00000-V32752 |
Step Relay | S0000-S8191 | S0000-S8176 |
Link Relay | B0000-B7FFF | B0000-B7FF0 |
Special Link Relay | SB000-SB7FF | SB000-SB7F0 |
Timer (Contact) | TS00000-TS23087 | --- |
Timer (Coil) | TC00000-TC23087 | --- |
Retentive Timer (Contact) | SS00000-SS23087 | --- |
Retentive Timer (Coil) | SC00000-SC23087 | --- |
Counter (Contact) | CS00000-CS23087 | --- |
Counter (Coil) | CC00000-CC23087 | --- |
Timer (Current Value) | --- | TN00000-TN23087 |
Retentive Timer (Current Value) | --- | SN00000-SN23087 |
Counter (Current Value) | --- | CN00000-CN23087 |
Data Register | --- | D00000-D25983 | *1
Special Register | --- | SD0000-SD2047 |
Link Register | --- | W0000-W657F |
Special Link Register | --- | SW000-SW7FF |
File Register (Normal) | --- | R00000-R32767 |
File Register (Serial) | --- | ZR0000000-ZR1042431 |
File Register (0R to 31R) | --- | 0R00000-0R32767 |
--- | 1R00000-1R32767 |
--- | 2R00000-2R32767 |
: | : | :
--- | 30R00000-30R32767 |
--- | 31R00000-31R26623 |

*1You can set the multi-CPU system in the system data area as well.

NOTE

- The address notation varies depending on the unit number you select.
  (Example) When "0" is selected for the unit number:
  (Example) When "1" is selected for the unit number:

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms