### 14A

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | COM port conversion adapter by Pro-face CA3-ADPCOM-01 |
(2) | Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 |
(3) | User-created cable Connector Display side: Terminal block External Device side: RJ-45 connector |

NOTE

- Please turn on the DIP Switch 1 to enable build-in resistance (100Ω) on the remotest External Device side.
- Cable length: 500m or less