### CutyAxis2 series

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Parameter | P000.00 - P046.31 | P000 - P046 | - | *1 *2
Point Table | PT00000.00 - PT00009.31 PT00100.00 - PT00109.31 PT00700.00 - PT00709.31 | PT00000 - PT00009 PT00100 - PT00109 PT00700 - PT00709 | *1 *3
Point Table (Continuation) | PTC00000.00 - PTC00009.31 PTC00100.00 - PTC00109.31 PTC00700.00 - PTC00709.31 | PTC00000 - PTC00009 PTC00100 - PTC00109 PTC00700 - PTC00709 | *1 *4 *5
Monitor | M00.00 - M17.31 | M00 - M17 | *1*6
IO monitor | IO0.00 - IO0.31 | IO |  | *1 *6 *7
Alarm | ALM0.00 - ALM8.15 | ALM0 - ALM8 | *6 *7
Mechanical Origin Rewriting | - | ZSET | - | *1 *7 *8
Positional Error Counter Set | - | ESET | *1 *7 *8
Point Table Selection | - | PNT |  | *7 *8
Emergency Stop | - | EMC | *7 *8
JOG Operation | - | JOG | *7 *8
Teaching | - | TDIN | *7 *8
Alarm Reset | - | ARST | *7 *8
Alarm History Clear | - | HCL | *7 *8
CPU Reset | - | RESET | *7 *8
EEPROM Writing | - | FLASH | *7 *8
Servo ON/OFF | SV | - | - | *7 *8
Point Table Start ON / OFF | STR | - | *7 *8
ZRTN Start-ON/OFF | ZSTR | - | *7 *8
Zero Slowdown LS ON/OFF | DEC | - | *7 *8
Input Branch ON/OFF | EXIN | - | *7 *8
HOLD-ON / HOLD-OFF | HOLD | - | *7 *8
Single-Block ON/OFF | SBK | - | *7 *8

*132-bit device. *2Usable parameter differs depending on the External Device. Refer to your External Device manual for details. *3Device address designation: *4Device address designation: *5In Point Table (Continuation) Device, reading and writing for the continuous addresses that extend from one point table number range to another can be specified. *6Write disabled. *7Command is assigned to each device. Refer to the table for the corresponding device and command. *8Read disabled.

##### Corresponding Device and Command

Device | Setting Value | Command | Function
--- | --- | --- | ---
IO | - | IO | The Status of IO
ALM0-ALM8 | - | ALM | Alarm Occurrence Situation
PNT | Point table No. | PNT | Point Table Selection
EMC | 0 | EMCON | Emergency Stop ON
1 or more | EMCOFF | Emergency Stop OFF
JOG | 0 | PJOG | Forward JOG
1 | NJOG | Reverse JOG
2 or more | JOGOFF | Suspending JOG operation
ZSET | Setting value | ZSET | Mechanical Origin Rewriting
ESET | Setting value | ESET | Position Error Counter Set
TDIN | Arbitrary value | TDIN | Teaching
ARST | Arbitrary value | ARST | Alarm Reset
HCL | Arbitrary value | HCL | Alarm History Clear
RESET | Arbitrary value | RESET | CPU Reset
FLASH | Arbitrary value | FLASH | EEPROM Writing
SV | SET | SVON | Servo ON
RESET | SVOFF | Servo OFF
STR | SET | STRON | Point Table Start ON
RESET | STROFF | Point Table Start OFF
ZSTR | SET | ZSTRON | ZRTN Start ON
RESET | ZSTROFF | ZRTN Start OFF
DEC | SET | DECON | Zero Slowdown LS ON
RESET | DECOFF | Zero Slowdown LS OFF
EXIN | SET | EXINON | Input Branch ON
RESET | EXINOFF | Input Branch OFF
HOLD | SET | HOLDON | HOLD-ON
RESET | HOLDOFF | HOLD-OFF
SBK | SET | SBKON | Single-Block On
RESET | SBKOFF | Single-Block OFF

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms