### Setting of External Device

Settings of the External Device vary depending on the connecting port.

##### When using the programmer connector on CPU

Select [PLC System Register Setting] from [Option] of the tool bar in the ladder software to display the [PLC System Register Setting] dialog box. Select the [Tool Port Setting] tab to set as below. Please refer to the manual of the External Device for more details.

Setup Items | Setting Value
--- | ---
Speed | 19200
Data Length | 8
Modem Connection | Disable
Not automatically change to 2400bps when connecting the modem | OFF
Unit No. | 1

##### When using the serial port connector on CPU

Select [PLC System Register Setting] from [Option] of the tool bar in the ladder software to display the [PLC System Register Setting] dialog box. Select the [COM Port Setting] tab to set as below. Please refer to the manual of the External Device for more details.

Setup Items | Setting Value
--- | ---
Speed | 19200
Data Length | 8
Parity | Odd
Stop Bit | 1
Operation Selection | Computer link
Modem Connection | OFF
Not automatically change to 2400bps | OFF
Unit No. | 1

NOTE

- Only FP-M (C20R/C20T/C32T) is equipped with the RS232C port. Other models are not.