### MicroLogix Series

Device | Bit Address | Word Address | 32 bit | Remarks
--- | --- | --- | --- | ---
Input File | I:00.000/00-I:08.255/15 | I:00.000-I08.255 |  | *1
Output File | O:00.000/00-O:08.255/15 | O:00.000-O:08.255 | *1
Status File | S:000/00-S:163/15 | S:000-S:163 |
Bit File | B003:000/00-B003:255/15 B009:000/00-B255:255/15 | B003:000-B003:255 B009:000-B255:255 |
Timer File | Enable | T004:000/-T004:255/ T009:000/-T255:255/ | EN | T004:000.-T004:255. T009:000.-T255:255. | - |
Timing | TT | -
Done | DN | -
Preset | - | PRE
Accumu-lated | - | ACC
Counter File | Up Enable | C005:000/-C005:255/ C009:000/-C255:255/ | CU | C005:000.-C005:255. C009:000.-C255:255. | - |
Down Enable | CD | -
Done | DN | -
Overflow | OV | -
Underflow | UN | -
Update Acc. | UA | -
Preset | - | PRE
Accumu-lated | - | ACC
Control File | Enable | R006:000/-R006:255/ R009:000/-R255:255/ | EN | R006:000.-R006:255. R009:000.-R255:255. | - |  |
Enable Unload | EU | -
Done | DN | -
Empty | EM | -
Error | ER | -
Unload | UL | -
Inhibit Comp. | IN | -
Found | FD | -
Length | - | LEN
Position | - | POS
Integer File | - | N007:000-N007:255 N009:000-N255:255 |
Floating Point File | - | F008:000-F008:255 F009:000-F255:255 | - | 32 Bit Access Only
String File | - | ST009:000-ST255:255 |  | *2
Long Word File | - | L009:000-L255:255 | - |

*1Input/Output File Address Designation is as shown below.

- Bit Designation

- Word Designation

*2The maximum length of the String File device is 82 bytes.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms