### 3G

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | Cable by YASKAWA CONTROLS CO., LTD FADHOWA-50 (0.5m) |

NOTE

- Example of cable image
  In the example above, the cable color is orange, and the identification mark shows red dot-line, which means TXD.
- Cable length: 30m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | ON