### MP3000 Series

Device | Bit address | Word address | 32 bits | Remarks
--- | --- | --- | --- | ---
Coil | GMB00000000 - GMB1048575F | GMB0000000 - GMB1048575 |  |
Input Relay | GIB000000 - GIB07FFFF | GIB00000 - GIB07FFF | *1 *2
GIB080000 - GIB0FFFFF | GIB08000 - GIB0FFFF | *1 *3
GIB100000 - GIB17FFFF | GIB10000 - GIB17FFF | *1 *2
Input Register | ----- | GIB00000 - GIB07FFF | *1 *2
GIB08000 - GIB0FFFF | *1 *3
GIB10000 - GIB17FFF | *1 *2
Hold Register | ----- | GMW0000000 - GMW1048575 |
Output Coil | GOB000000 - GOB07FFFF | GOB00000 - GOB07FFF | *4
GOB080000 - GOB0FFFFF | GOB08000 - GOB0FFFF | *3
GOB100000 - GOB17FFFF | GOB10000 - GOB17FFF | *4
Output Register | ----- | GOB00000 - GOB07FFF | *4
GOB08000 - GOB0FFFF | *3
GOB10000 - GOB17FFF | *4
Data Relay | GGB000000000 - GGB16777215F | GGB00000000 - GGB16777215 |
Data Register | ----- | GGW00000000 - GGW16777215 |
System Register | SB000000 - SB65534F | SW00000 - SW65534 |

*1Write disable

*2Input area

*3Motion parameter. The address format is shown below.

bit | 15 | 14-11 | 10-7 | 6-0
Description | 1 (Fix) | value of "Line number - 1" | value of "Axis number - 1" | Address (0x00 - 0x7F)

*4Output area

The Display address is equivalent to the matching External Device address plus the offset. Addresses in the system register are equivalent between the Display and External Device.

The following shows the relationship of addresses between the Display and External Device.

Device | Display on BLUE | Display on External Device
--- | --- | ---
Coil (Bit device) | GMB00000000 - GMB1048575F | MW00000000+Offset - MW1048575F+Offset
Coil (Word device) | GMB0000000 - GMB1048575 | MW0000000+Offset - MW1048575+Offset
Input Relay (Bit device) | GIB000000 - GIB17FFFF | IW000000+Offset - IW17FFFF+Offset
Input Relay (Word device) | GIB00000 - GIB17FFF | IW00000+Offset - IW17FFF+Offset
Input Register | GIW00000 - GIW17FFF | IW00000+Offset - IW17FFF+Offset
Hold Register | GMW0000000 - GMW1048575 | MW0000000+Offset - MW1048575+Offset
Output Coil (Bit device) | GOB000000 - GOB17FFFF | OW000000+Offset - OW17FFFF+Offset
Output Coil (Word device) | GOB00000 - GOB17FFF | OW000000+Offset - OW17FFFF+Offset
Output Register | GOW00000 - GOW17FFF | OW000000+Offset - OW17FFFF+Offset
Data Relay (Bit device) | GGB000000000 - GGB16777215F | GW000000000+Offset - GW16777215F+Offset
Data Relay (Word device) | GGB00000000 - GGB16777215 | GW00000000+Offset - GW16777215+Offset
Data Register | GGW00000000 - GGW16777215 | GW00000000+Offset - GW16777215+Offset

e.g) When you specify "GMW00000" in BLUE, the address of "MW00000" to which offset value is added, is specified as the actual address in the External Device. Offset value is described as "Head REG" in the ladder software.

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms