### PLC-5 Series

Device | Bit Address | Word Address | 32bits | Remarks
--- | --- | --- | --- | ---
Input File | I:0/0 - I:377/17 | I:0 - I:377 |  |
Output File | O:0/0 - O:377/17 | O:0 - O:377 |
Status File | S:0/0 - S:163/15 | S:0 - S:163 |  |
Bit File | B3:0/0 - B999:999/15 | B3:0 - B999:999 |  |
Timer File | Enable | T3:0/ - T999:999/ | EN | T3:0. - T999:999. | - |  |
Timing | TT | - |
Done | DN | - |
Preset | - | PRE |
Accumulated | - | ACC |
Counter File | Up Enable | C3:0/ - C999:999/ | CU | C3:0. - C999:999. | - |
Down Enable | CD | - |
Done | DN | - |
Overflow | OV | - |
Underflow | UN | - |
Update Acc | UA | - |
Preset | - | PRE |
Accumulated | - | ACC |
Control File | Enable | R3:0/ - R999:999/ | EN | R3:0. - R999:999. | - |
Enable Unload | EU | - |
Done | DN | - |
Empty | EM | - |
Error | ER | - |
Unload | UL | - |
Inhibit Comp. | IN | - |
Found | FD | - |
Length | - | LEN |
Position | - | POS |
Integer File | N3:0/0 - N999:999/15 | N3:0 - N999:999 |  |
Floating Point File | ------ | F3:0 - F999:999 |  | 32-bit address only
String File | ------ | ST3:0 - ST999:999 |  |
ASCII File | A3:0/0 - A999:999/15 | A3:0 - A999:999 |  |
BCD File | D3:0/0 - D999:999/15 | D3:0 - D999:999 |

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms