### 3E

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | User-created cable • Connector Display side: Terminal block External Device side: Terminal block |

NOTE

- The cable length have to be 500m or less. When using FX1N-485-BD, FX2N-485-BD, FX3U-485-BD or FX3G-485-BD, the cable length have to be 50m or less.

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | ON
2 | OFF
3 | ON
4 | OFF