### Setting of External Device

Use the programming software (FPWIN GR7S v2.7.0.0) to set up communication settings on the External Device. For details on communication settings, please refer to the manual of the External Device.

1. Start up the programming software.

2. Select the series for the External Device.

3. Click [OK] to display a new project.

4. From the menu bar, select [Option].

5. Select [FP7 Configuration]-[Built-in SCU].

6. Click the port you want to use (COM0, COM1 or COM2).

7. Set the each item as follows, and click [OK].

Setup Items | Setting Value
Communication mode | MEWTOCOL-7
Station No. | 1
Baud rate | 9600bps
Data length | 8 bits
Parity | Odd
Stop bit | 1 bit
RS/CS | Disable
Send waiting time | 0
Header STX | Disable
Terminator setting | CR
Modem initialization | Not initialize