### SPH5000M (NP1PA1-512E)

Device | Bit Address | Word Address | 32bits | Remarks
--- | --- | --- | --- | ---
Input Memory | %IX□.0000.00 - %IX□.0511.15 | %IW□.0000 - %IW□.0511 |  | *1
Output Memory | %QX□.0000.00 - %QX□.0511.15 | %QW□.0000 - %QW□.0511 | *1
Standard Memory | %MX□.1.00000000.00- %MX□.1.02097151.15 | %MW□.1.00000000- %MW□.1.02097151 | *2 *3
CPU Common Standard Memory | %MX□.1.02097152.00- %MX□.1.07340031.15 | %MW□.1.02097152- %MW□.1.07340031 | *2 *3
Multiple CPU Standard Memory (for enhanced processor bus) | %MX□.1.15728640.00- %MX□.1.16515071.15 | %MW□.1.15728640- %MW□.1.16515071 | *2 *3
Multiple CPU Standard Memory (for processor bus) | %MX□.1.16515072.00- %MX□.1.16646143.15 | %MW□.1.16515072- %MW□.1.16646143 | *2 *3
APL0/APL1 Standard Memory | %MX*.□.1.00000000.00- %MX*.□.1.02097151.15 | %MW*.□.1.00000000- %MW*.□.1.02097151 | *4
Retain Memory | %MX□.3.00000000.00- %MX□.3.01048575.15 | %MW□.3.00000000- %MW□.3.01048575 | *2 *3
CPU Common Retain Memory | %MX□.3.02097152.00- %MX□.3.03145728.15 | %MW□.3.02097152- %MW□.3.03145728 | *2 *3
Multiple-CPU Retain Memory (for enhanced processor bus) | %MX□.3.15728640.00- %MX□.3.16515071.15 | %MW□.3.15728640- %MW□.3.16515071 | *2 *3
Multiple CPU Retain Memory (for processor bus) | %MX□.3.16515072.00- %MX□.3.16646143.15 | %MW□.3.16515072- %MW□.3.16646143 | *2 *3
APL0/APL1 Retain Memory | %MX*.□.3.00000000.00- %MX*.□.3.01048575.15 | %MW*.□.3.00000000- %MW*.□.3.01048575 | *4
System Memory | %MX□.10.0000000.00- %MX□.10.0000511.15 | %MW□.10.0000000- %MW□.10.0000511 | *2
System Memory (for APL0/APL1, E-SX bus) | %MX*.□.10.0000000.00- %MX*.□.10.0000511.15 | %MW*.□.10.0000000- %MW*.□.10.0000511 | *4
System Memory (E-SX bus assembly) | %MX*.□.10.0000512.00- %MX*.□.10.0016895.15 | %MW*.□.10.0000512- %MW*.□.10.0016895 | *4

*1Input/Output Memory Address Designation is as shown below.

- Bit Designation

- Word Designation

NOTE

- Please Refer to the SX Bus Unit no. details in the manual of External Device.

*2Standard/Retain/System Memory Address Designation is as shown below.

- Bit Designation

- Word Designation

*3Standard and Retain Memory sizes can be changed. However, the total memory size is fixed. (For details, refer to the manual of External Device).

*4APL0/APL1 Standard/Retain/System Memory Address Designation is as shown below.

- Bit Designation

- Word Designation

NOTE

- Please Refer to the SX Bus Unit no. details in the manual of External Device.

NOTE

- When specifying the address of the External Device directly, always use a setting within the specified AT range of the ladder software. We recommend using an AT-specified- variable for the External Device used on the Display. Please refer to the MICREX-SX Series D300Win <Reference> Users Manual by Fuji Electric Co., Ltd. for details of specifying the AT range and how to set it. When using a variable that is not AT-specified, variable needs to be imported again and screen transfer needs to be executed if ladder program or variable is changed.
- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms