Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | 00000 - 59915 | 000 - 599 |  |
Output Relay |
Internal Auxiliary Relay |
Control Relay | CR0000 - CR3915 | CR00 - CR39 |
Timer (Contact) | T000 - T511 | ------ | - |
Counter (Contact) | C000 - C511 | ------ |
High-speed Counter Comparator (Contact) | CTC0 - CTC3 | ------ | *1
Timer (Setting Value) | ------ | TS000 - TS511 |  | *2
Counter (Setting Value) | ------ | CS000 - CS511 | *2
Timer (Current Value) | ------ | TC000 - TC511 | *2
Counter (Current Value) | ------ | CC000 - CC511 | *2
Data Memory | ------ | DM00000 - DM39999 |
Temporary Data Memory | ------ | TM000 - TM511 |
Control Memory | ------ | CM0000 - CM3999 |
Digital Trimmer | ------ | TRM0 - TRM7 | *2
High-speed Counter (Current Value) | ------ | CTH0 - CTH1 | *2
High-speed Counter Comparator (Setting Value) | ------ | CTC0 - CTC3 | *2

*1Write disable

*232-bit device

IMPORTANT:

- When connecting KV-700 Series, use settings within the device address ranges above.
- If you try to access device addresses supported only by the KV-1000 Series devices, the following error messages display: "Error has been responded for device read command (Error Code(02)[(0x02)]" or "Error has been responded for device write command (Error Code(02)[(0x02)]".

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms